# Darlington Driver Chip Page 17

## Used with the LED Bar





 The LEDs are in a Dual in-line (DIL) integrated package.
 The eight resistors are in a Single in-line (SIL) integrated package.
 The discrete component diode is for polarity protection.
 The ULN2803A is an 18 pin DIL integrated circuit (IC).