**Op Amps - Key Facts**

|  |
| --- |
| **Ideal Op Amp**Summary-op-amp.gif |
| Gain | Infinity |
| Input resistance | Infinity |
| Output resistance | Zero |
| Gain Bandwidth Product (GBP) | InfinityGain x Frequency = GBP |

|  |
| --- |
| **Comparator**Summary-comparator.gif |
| Gain | Infinity |
| Output | Always saturated high or low |
| Input Resistance | Infinity |
| Comparisons | * If V+ is greater than V- then the output is high.
* If V+ is less than V- then the output is low.
 |

|  |
| --- |
| **Inverting Amplifier**Summary-Inverting.gif |
| Gain | * Gv = -Rf / R1
* Gv = Vout / Vin
 |
| Input resistance | R1 |
| Virtual Earth | Point POp Amps have a very high open loop gain so if the output is a few volts, the inverting input voltage will be a few microvolts. This is so close to zero, it is called a virtual earth. |

|  |
| --- |
| **Non Inverting Amplifier - Two Ways to Draw the Diagram**Summary-Non-Inverting.gif Non Inverting - Alternative Diagram |
| Gain | * Gv = 1 + Rf / R1
* Gv = Vout / Vin
 |
| Input resistance | The input resistance of the op amp which is roughly infinity. |

|  |
| --- |
| **Summing Amplifier**Summary-Summing-Inverting.gif |
| Calculate Vout | Vout = - Rf (V1/R1 + V2/R2 + V3/R3) |
| Input resistance | It's R1 for the V1 input and R2 for the V2 input etc. |
| Virtual Earth | The point P is the virtual earth. |

|  |
| --- |
| **Difference Amplifier**Summary-difference-amplifier.gif |
| Calculate Vout | Vout = ( V+ - V- ) x ( Rf / R1 ) |
| Input Resistance | 2 x R1 |

|  |
| --- |
| **Voltage Follower**Summary-voltage-follower.gif |
| Voltage Gain | The voltage gain is ONE. |
| Power and Current Gain | This can be very large. |
| Input resistance | Infinity |
| Output resistance | Small so usefully large currents can be provided. |
| **Schmitt Trigger**Op Amp Inverting-Schmitt-Trig.gif* On the left, a simple version with positive feedback giving different on and off reference voltages.
* On the right is a comparator with one extra resistor giving positive feedback to give different on and off reference voltages.
 |