
**4017 with OR Page 37**



**This shows how OR gates can be used to control an event such as a buzz which repeats at specified time intervals.**

**A MOSFET driver is needed between the OR gates and the buzzer or other device.**

**Use a 7432 quad OR chip. This runs on 5 Volts so the rest of the circuit should also be run on 5V.**